E350 / F150 Instrument Panel Connections

C250 – BROWN/BLACK (a)  
	Pin
	93 Wire
	Use
	New
	Tach vers
	

	1
	-
	-
	fm B11
	LG/R
	Charge out

	2
	GY/W
	High beam
	"
	"
	"

	3
	BK
	Gnd
	"
	"
	"

	4
	DG/LG
	Fasten Belt
	"
	"
	"

	5
	-
	-
	fm B6
	Y/W
	Fuel w/tach

	6
	LB/R
	Panel Lites
	"
	"
	"

	7
	BK
	Gnd
	"
	"
	"

	
	
	
	
	
	

	8
	W/LB
	Right turn
	"
	"
	"

	*9*
	O/BK
	Trans temp
	fm ICM
	W/PK
	Tach in

	10
	BK/Y
	Airbag
	fm A12
	"
	Tach V8 flag

	*11*
	R/Y
	Pwr
	x
	LB/BK
	Low range

	*12*
	BK/W
	Gnd fi
	x
	LB
	4x4

	13
	-
	-
	fm A11
	R/Y
	Pwr Run+Start

	*14*
	BK/W
	Gnd volt
	fm B12
	R/LG
	Charge in


C251 – GREY (b)
	Pin
	93 Wire
	Use
	New
	Tach vers
	

	1
	-
	-
	fm A14
	BK/LB
	Gauge gnd

	2
	-
	-
	fm B5
	PK/LG
	Check Engine

	3
	DG
	ABS
	"
	"
	"

	4
	P/W
	Brake
	"
	"
	"

	*5*
	PK/LG
	Check engine
	x
	DB/LG
	Anti-theft

	*6*
	Y/W
	Fuel (no tach)
	-
	-
	-

	7
	LG/W
	Left turn
	"
	"
	"

	
	
	
	
	
	

	8
	W/R
	Oil pressure
	"
	"
	"

	9
	BK/W
	Gnd
	"
	BK/LB
	"

	10
	R/W
	Temp
	"
	"
	"

	*11*
	LG/R
	Charge out
	-
	-
	-

	*12*
	R/LG
	Charge in
	x
	BK/Y
	Airbag

	13
	R/Y
	Gauge pwr
	"
	"
	"

	14
	-
	-
	fm B13
	-
	Anti-slosh mod


New = "" if stays same,    
"x" if cut,    
"-" if no connection,

"fm xxx" if jumpered from different input wire

ICM (under starter solenoid) for PIP




	TAN/Y
	Coil

	 PK
	SPOUT

	GY/O
	PIP (to tach)

	R/LG
	Pwr

	BK/W
	Gnd


MY NOTES:

Apparently the 92-93 E/F van/truck swaps with only a couple of wires, and the same for 94-96.   But if you mix the year eras, you end up with having to swap more wires like I did.

OLD NOTES FROM SOMEONE ELSE:


[image: image1.emf]Looking at the plug straight on the bottom row of pins are numbered 1 - 7 going  left to right. The top row goes the right to left with numbers 8 - 14.     The LG/R wire #904 moves from location 11 in its orginal plug to number 1 on  the other plug. Number 12 on th e same plug is R/LG #16 must move to  Number 14 on the other plug. Number 14 moves to number 13 on that plug.  Numbers 2 and three must be reversed in the original plug.     So two wires move to the other plug Number 16 R/LG goes from 12 to 14 and  Number 11 pin  moves to number 1 pin on the other plug Circuit 904 LG/R.       A 1994 or 1995 cluster will not charge the   battery   when put in a 1992 or 1993  gas truc k.   To make it charge you have to swap wires between the two plugs.  
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Looking at the plug straight on the bottom row of pins are numbered 1-7 going left to right. The top row goes the right to left with numbers 8-14.

The LG/R wire #904 moves from location 11 in its orginal plug to number 1 on the other plug. Number 12 on the same plug is R/LG #16 must move to Number 14 on the other plug. Number 14 moves to number 13 on that plug. Numbers 2 and three must be reversed in the original plug.

So two wires move to the other plug Number 16 R/LG goes from 12 to 14 and Number 11 pin moves to number 1 pin on the other plug Circuit 904 LG/R.

A 1994 or 1995 cluster will not charge the battery when put in a 1992 or 1993 gas truck.
To make it charge you have to swap wires between the two plugs.
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